modbus\_tcp\_pi\_accept(3)

=======================

NAME

----

modbus\_tcp\_pi\_accept - accept a new connection on a TCP PI Modbus socket (IPv6)

SYNOPSIS

--------

\*int modbus\_tcp\_pi\_accept(modbus\_t \*'ctx', int \*'s);\*

DESCRIPTION

-----------

The \*modbus\_tcp\_pi\_accept()\* function shall extract the first connection on the

queue of pending connections, create a new socket and store it in libmodbus

context given in argument. If available, \_accept4()\_ with `SOCK\_CLOEXEC` will be

called instead of \*accept()\*.

RETURN VALUE

------------

The function shall return a new socket if successful.

Otherwise it shall return -1 and set errno.

EXAMPLE

-------

For detailed example, see unit-test-server.c source file in tests directory.

[source,c]

-------------------

...

ctx = modbus\_new\_tcp\_pi("::0", 502);

s = modbus\_tcp\_pi\_listen(ctx, 1);

modbus\_tcp\_pi\_accept(ctx, &s);

...

close(s)

modbus\_free(ctx);

-------------------

SEE ALSO

--------

linkmb:modbus\_tcp\_pi\_accept[3]

linkmb:modbus\_tcp\_listen[3]

linkmb:modbus\_tcp\_pi\_listen[3]

AUTHORS

-------

The libmodbus documentation was written by Stéphane Raimbault

<stephane.raimbault@gmail.com>