modbus\_rtu\_get\_rts\_delay(3)

===========================

NAME

----

modbus\_rtu\_get\_rts\_delay - get the current RTS delay in RTU

SYNOPSIS

--------

\*int modbus\_rtu\_get\_rts\_delay(modbus\_t \*'ctx');\*

DESCRIPTION

-----------

The \_modbus\_rtu\_get\_rts\_delay()\_ function shall get the current Request To Send

delay period of the libmodbus context 'ctx'.

This function can only be used with a context using a RTU backend.

RETURN VALUE

------------

The \_modbus\_rtu\_get\_rts\_delay()\_ function shall return the current RTS delay in

microseconds if successful. Otherwise it shall return -1 and set errno.

ERRORS

------

\*EINVAL\*::

The libmodbus backend is not RTU.

SEE ALSO

--------

linkmb:modbus\_rtu\_set\_rts\_delay[3]

AUTHORS

-------

Jimmy Bergström <jimmy@ekontroll.com>

The libmodbus documentation was written by Stéphane Raimbault

<stephane.raimbault@gmail.com>